bvets vehicle sound 3.01

[Flange]
0  = Noize\Flange0.wav		; 標準
1  = Noize\Flange1.wav		; 低速（仮）

[Run]
0  = Tc\Run_25mN.wav		; 25mジョイント
1  = Tc\Run_bridge.wav		; 鉄橋
2  = Tc\Run_bridge2.wav		; 小鉄橋
3  = Tc\Run_tunnel25.wav	; トンネル25mジョイント
4  = Tc\Run_tunnellong.wav	; トンネルロング
;5  = Tc\Run_joint.wav		; ジョイント（使用非推奨）
6  = Tc\Run_slablong.wav	; スラブロング
7  = Tc\Run_long.wav		; ロング
8  = Tc\Run_long_kin.wav	; ロング鳴り
9  = Tc\Run_25mN2.wav		; 25mジョイント（強）

[Ats]
0  = ATS\Ats.wav
1  = ATS\AtsCnt.wav
2  = ATS\ATSbellReverb.wav
10  = ATS\Halt.wav
113  = ATS\EB.wav
180 = ATS\BuzzerP.wav
181 = ATS\Buzzer.wav
190 = ATS\cutting_a_breaker.wav
98 = otologic\Light_Switch-Selector_Button01-1(Dry-Mid).wav

182 = Door\DoorAnIn_chiku.wav
183 = Door\DoorAnO_chiku.wav
;182 = Door\DoorAnIn_kako.wav
;183 = Door\DoorAnO_kako.wav

150 = ATS\DK\DK150.wav
151 = ATS\DK\DK151.wav
152 = ATS\DK\DK152.wav
153 = ATS\DK\DK153.wav
154 = ATS\DK\DK154.wav
155 = ATS\DK\DK155.wav
156 = ATS\DK\DK156.wav

140 = Door\DoorOpnL.wav
141 = Door\DoorOpnR.wav
142 = Door\DoorClsL.wav
143 = Door\DoorClsR.wav
145 = Door\cover_openL.wav
146 = Door\cover_openR.wav
147 = Door\cover_closeL.wav
148 = Door\cover_closeR.wav

;;ptpt.DLL
205 = Noize\kazekiri.wav

;;Shock.DLL
160 = Noize\shock817.wav	;ノイズ1
161 = Noize\shock817.wav	;ノイズ1
162 = Noize\shock817.wav	;ノイズ1
163 = Noize\shock817.wav	;再加速ノイズ
;164 = Noize\			;停車時ノイズ（強）
;165 = Noize\			;停車時ノイズ（弱）

[Switch]
0   = Switch\Point.wav		;低速分岐Point1
1   = Switch\Point2.wav	        ;低速分岐Point2
2   = Switch\Point3.wav	        ;高速通過Point
4   = Switch\joint_slab.wav	;スラブJoint
5   = Switch\joint.wav		;Joint
6   = Switch\fm1.wav		;踏切1
7   = Switch\fm2.wav		;踏切2


[Motor]



[Brake]
BC Release High		= Brake\Airhigh3.wav	; ゆるめ (高圧)
BC Release		= Brake\Air.wav		; ゆるめ
BC Release Full		= Brake\AirZero2.wav	; 全ゆるめ
Emergency		= Brake\EmrBrake.wav	; 非常

[Master Controller]
Max		 = mascon2\p_high2.wav
Up		 = mascon2\p1.wav
UpFast		 = mascon2\p_fast2.wav
Down 		 = mascon2\p1.wav
DownFast	 = mascon2\p_fast2.wav
Min 		 = mascon2\p_off.wav

[Brake Handle]
Min		 = mascon2\br_off.wav
Apply		 = mascon2\br_on.wav
ApplyFast	 = mascon2\br_on2.wav
Release		 = mascon2\br1.wav
ReleaseFast	 = mascon2\br_fast62.wav
Max 		 = mascon2\br_highBC.wav

[Reverser]
;On = mascon2\RV_on Mc.wav			; Mc用
On = mascon2\RV_on.wav				; Tc用
Off = mascon2\RV_off.wav


[Compressor]
;815/817Mcでは使用しない

;815/817Tc
Release 	 = Tc\CPEnd.wav
Loop 		 = Tc\CPLoop.wav
Attack		 = Tc\CPStart.wav

;817Tc-ScreenCP
;Loop 		 = Tc\CPLoop_screen.wav
;Attack 		 = Tc\CPStart_screen.wav

[Horn]
Primary  = KlaxonLP.wav
PrimaryRelease  = KlaxonRS.wav

;Secondary  = Door\DoorAn_kako.wav		;カコ車アナウンス
Secondary  = Door\DoorAn_chiku.wav		;それ以外

[Suspension]
Left  = Noize\SpringL.wav
Right  = Noize\SpringR.wav
LeftApply  = Noize\LeftApply.wav
RightApply  = Noize\RightApply.wav

[Others]
Noise  = Noize\Loop.wav
Shoe  = Noize\Rub.wav
;Shoe  = Noize\Rub1.wav
